{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["河段主要指标"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"河段主要指标","index":0,"n_rows":4,"n_cols":63,"rows_kept":4,"merged":[[0,0,0,62],[1,0,1,62]],"flags":["formulas_cached_only"]}
["河段主要指标报表","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","",""]
["导出人:admin","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","",""]
["河（渠）名称","选择河段","防洪标准现状","设计防洪标准","规划防洪标准","防洪水位现状","设计防洪水位","规划防洪水位","相应防洪流量现状","设计防洪流量","规划防洪流量","排涝标准现状","排涝标准设计","排涝标准规划","排涝水位现状","设计排涝水位","规划排涝水位","排涝流量现状","设计排涝流量","规划排涝流量","河底比降现状","设计河底比降","规划河底比降","河底高程现状（m）","设计河底高程（m）","规划河底高程（m）","河道底宽现状（m）","设计河道底宽（m）","规划河道底宽（m）","河道（堤防）左岸边坡现状","河道（堤防）左岸边坡设计","河道（堤防）左岸边坡规划","河道（堤防）右岸边坡现状","河道（堤防）右岸边坡设计","河道（堤防）右岸边坡规划","左岸堤顶高程现状（m）","左岸堤顶高程设计（m）","左岸堤顶高程规划（m）","右岸堤顶高程现状（m）","右岸堤顶高程设计（m）","右岸堤顶高程规划（m）","左岸堤顶宽度现状（m）","左岸堤顶宽度设计（m）","左岸堤顶宽度规划（m）","右岸堤顶宽度现状（m）","右岸堤顶宽度设计（m）","右岸堤顶宽度规划（m）","左岸堤外地面高程现状（m）","左岸堤外地面高程设计（m）","左岸堤外地面高程规划（m）","右岸堤外地面高程现状（m）","右岸堤外地面高程设计（m）","右岸堤外地面高程规划（m）","输水流量现状","设计输水流量","规划输水流量","输水水位现状","设计输水水位","规划输水水位","其他指标现状","其他指标设计","其他指标规划","断面桩号"]
["马颊岔河","渠道",null,"61年雨型",null,null,19.46,null,null,360,null,null,"64年雨型",null,null,18.25,null,null,150,null,null,"1/11200",null,null,14.21,null,null,60,null,"无堤防","01:03:00",null,"01:03:00","01:03:00",null,null,21.46,null,19.3,21.46,null,null,6,null,19,6]